**DELHI DEVELOPMENT AUTHORITY**

# **HARI NAGAR SPORTS COMPLEX**

No. F.7(11)08-09/CW/HNSC/526 Dt. : 15.07.08

# **NOTICE INVITING QUOTATION­ No. 5**

Sealed item rate quotations are hereby invited on behalf of DDA by the Secretary, HNSC. The quotation should reach in the office of the undersigned on or before 25.07.08 up to 3.00 p.m. and the same shall be opened on the same day at 3.30 p.m. in the presence of the intending quotationers & their representatives.

Name of work: - M/o HNSC DDA

SH: Renovation of Toilets in Multigym at Pratap Nagar (As per scheduled attached)

**Conditions:**

1. The work/supply should be done at HNSC.
2. The Agency should be professional.
3. The work/supply should be done as per specification.
4. Nothing extra shall be paid.
5. The payment will be made to the agency after the entire satisfaction of Secretary (HNSC) / JE (Civil), HNSC.
6. The undersigned reserves the right to reject /accept the lowest quotations without assigning any reason.
7. The Agency will be responsible for any loss of materials / damage due to negligence.
8. Conditional quotations will not be entertained.
9. The time allowed for execution of the work is 45 days from the date of issue of the work order.
10. The rates shall be inclusive of all taxes including statutory liabilities.
11. Agency should be registered with Trade & Taxes GNCT of Delhi and supposed to furnish a copy of TIN and clearance certificate on Quarterly basis otherwise Quotation may not be considered.
12. Validity of quotation shall be 60 days from the date of opening.

Secretary (HNSC)

CC:

1. Director (Sports).
2. Director (System) with the request to bring the NIQ on DDA’s Web-site through Email- ddatender@dda.org.in.
3. Sr. A.O (Sports).
4. Secretary all sports complexes.
5. A.A.O (HNSC)
6. DDA Contractor Association, Vikas Kutir Room no. 12, Bkno.1, New Delhi.
7. The Secy., DDA Builders Association F-18, Vikas Mina, ITO, New Delhi.
8. DDA Contractor Association E-18 Vikas Kutir, ITO, New Delhi.
9. Notice Board.
10. Guard file

Secretary (HNSC)

**DELHI DEVELOPMENT AUTHORITY**

# HARI NAGAR SPORTS COMPLEX

Name of work :- M/o Hari Nagar Sports Complex

**SH : Renovation of toilets in Multi-Gym at Partap Nagar.**

|  |  |  |  |
| --- | --- | --- | --- |
| **Sr. No.** | **Description of Items** | **Qty** | **Unit** |
| 1. | Dismantling tile work in floors and roofs laid in cement mortar including stacking material within 50 m lead.   1. For thickness of tiles 10 mm to 25 mm. | 59.00 | Sqm. |
| 2. | Providing fixing Ist quality ceramic glazed floor tiles conforming to ISI : 13753 of minimum thickness 5 mm of approved make like NITCO, ORIENT, KAJARIA, SOMANY or equivalent make in all colours, shades except begundy, bottle green, of any size as approved by Engineer-in-charge in skirting, risers of steps and dados over 12 mm thick bed Cement Mortar 1:3 (1 Cement : 3 Coarse sand) and jointing withgrey cement slurry @ 3.3 Kg per sqm including pointing in while cement mixed with pigment of matching shade complete. | 59.00 | Sqm. |
| 3. | Half brick masonry with bricks of class designation 75 in  Foundation and plinth in:   1. Cement mortar 1: 4 (1 Cement : 4 Coarse sand | 3.00 | Sqm. |
| 4. | 1. mm cement plaster of mix   b) 1: 4 (1 Cement : 4 fine sand | 19.00 | Sqm. |
| 5 | Providing and laying ceramic glazed floor tiles 300 X 300 mm (thickness to be specified by the manufacture) of 1st quality conforming to ISI : 13755 of NITCO, ORIENT, KAJARIA, SOMANY or equivalent make / colours, such as white, Ivory, Grey, Fume Red Brown laid on 20 mm thick Cement Mortar 1:4 (1 Cement : 4 Coarse sand) including pointing the joints with white cement and matching pigment etc. complete. | 17.00 | Sqm. |
| 6 | Supplying of tiles adhesive for the fixing of tile of approved manufacture @ 8.57 sqm as per the direction of Engineer in charge. | 146.00 | Kg |
| 7 | Providing and fixing ISI marked flush door shutters non decorative type, core of block board construction with frame of 1st class hard wood and well matched commercial 3 ply veneering with vertical grains or cross bands and face vaneers on both faces of shutters.  (b) 35 mm thick including ISI marked stainless steel butt hinges with necessary screws. | 9.25 | Sqm. |
| 8 | Providing and fixing water closet squatting pan (Indian type WC Pan) with 100 mm sand cast iron P or S trap, 10 liter low level white PVC flushing cistern with manually controlled device (handle level) confirming to IS : 7231 Parryware / Hindware / Seabird / Orient (Coral) with all fittings and fixtures complete including cutting and making good the walls and floors wherever required.  (a) White Vitreous china Orrisa pattern WC pan of size 580 X 440 mm with integral type foot rests. | 1 No. | Each |
| 9 | Providing & fixing white vitreous china pedestal type water closet (European type) with seat and lid, 10 liter low level white PVC Flushing cistern with manually controlled device (handle lever) confirming to IS : 7231 Parryware / Hindware ? Seabird / Orient (Coral) with fittings and fixtures complete including cuttings and making good the walls and floors whenever required.  (b) W C pan with ISI marked black solid seat and lid. | 1 No. | Each |
| 10 | Providing and fixing wash basin with C I / M S brackets, 15 mm C P Brass pillar, Kingston / Gem / techno / Parko, 32 mm C P brass waste of standard pattern, including painting of fittings and brackets cutting and making good the walls wherever require :  (b) Flat back wash basin size 550 X 400 mm with single 15 mm C P brass pillar tap. | 2 Nos. | Each |
| 11 | Providing and fixing white vitreous china flat back half stall urinal of 850 X 380 X 350 mm with PVC automatic flushing cistern, Parryware / Hindware / Seabird / Orient (Coral) with fittings, standard size C P Brass flush pipe, spreaders with unions and clamps (all in C P brass) with waste fittings as per IS : 2556, C I Trap with outlet grating and other couplings in C P Brass including painting of fittings and cutting and making good the walls and floors whenever required.  (b) Range of two half stall urinals with 5 liters PVC automatic flushing cistern. | 1 No. | Each |
| 12 | Providing and fixing poly carbonate 6 mm thick sheet coloured of required shade roofing and fixing with J & L hooks bolts and nuts and washer etc complete. | 16.00 | Sqm. |
| 13 | Renewing glass panes with putty and nails where ever necessary   1. Glass panes weighting 10 Kg / sqm. | 7.00 | Sqm. |
| 14 | Removing white or colour wash by scrapping and sand papering and preparing the surface smooth including necessary repairs to scratches etc as complete. | 87.00 | Sqm. |
| 15 | Distempering with oil bound washable distemper of approved brand and manufacture to give an even shade.   1. New Work (two or more coats) over & i/c primary coat with cement primer. | 87.00 | Sqm. |
| 16 | Painting with Synthetic enamel paint of approved brand and manufacture of required colour to give an even shade.   1. Two or more coats on new work. | 28.00 | Sqm. |
| 17 | Providing & fixing CP Brass angle valve for basin mixer and gyser points of approved quality confirming to IS : 8931.   1. 15 mm nominal bore. | 6 No. | Each |
| 18 | P/F CP Brass bib cook of approved quality confirming to IS : 8931.   1. 15 mm nominal bore. | 4 Nos. | Each |
| 19 | P/F unplasticised PVC connection pipe with brass unions.   1. 45 mm length 15 mm nominal bore. | 6 Nos. | Each |
| 20 | P/F PTMT Bottle trap of wash basin and sink ( Paryagor equivalent)   1. Bottle trap 38 mm single piece moulded with height of 270 mm effective length of tail piece 265 mm from the centre of the waste compiling 77 mm breadth with 25 mm minimum water seal weighting not less than 270gm. | 2 Nos. | Each |
| 21 | Marble work (table rubbed and polished) for wall lining (veneer work) in CM 1:3 (1 Cement : 3 C. sand) i/c pointing with CM 1:2 (1 Cement : 2 marble dust) with an admixture of pigment to match the marble shade ( to be secured to the backing by means of cramps, which shall be paid for separately)   1. White marble – Raj Nagar plain 18 mm thick (over 0.2 sq mt. but upto 0.5 sq mt.) | 1.50 | Sq mt. |
| 22 | P/F 600 X 450 mm beveled edge mirror of superior glass (of approved quality) complete with 6 mm thick hard board ground fixed to wooden cleats with CP Brass screws and washers complete. | 2 No. | Each |
| 23 | Providing and placing on terrace (at all floor levels) polyethylene water storage tank ISI : 12701 marked indicating the BIS license No. with corner & suitable locking arrangement and making necessary holes for inlet, outlet and overflow pipes but without fittings and the base support for tank (sintex, electric plast, star, lotus or equivalent having valid license No.) | 1000.00 | Per lit. Capacity |
| 24 | P/L in position cement coversite of specified grade i/c the cost of centing & shutting all work up to plinth level.   1. 1:5:10 (1 Cement : 5 C. sand : 10 Graded stone agg 40 mm) 2. 1:2:4 (1 Cement : 2 C.sand : 4 Graded stone agg 20 mm N. size) | 0.50  0.25 | Cu.m.  Cu.m. |
| 25 | Kota stone slab flooring over 20 mm ( average) thick base land over and jointed with grey cement slurry mixed with pigment to match the shade of the slab i/c rubbing and polishing complete with bore of 1 : 4 (1 Cement : 4 C. sand).   1. 25 mm thick | 31.0 | Sq. mt. |

**Secretary (HNSC) JE (C)**