**DELHI DEVELOPMENT AUTHORITY**

# **HARI NAGAR SPORTS COMPLEX**

No. F.7(11)08-09/CW/HNSC/537 Dt. : 25/07/08

# **NOTICE INVITING QUOTATION­ No. 08/2008-09**

Sealed item rate quotations are hereby invited on behalf of DDA by the Secretary, HNSC. The quotation should reach in the office of the undersigned on or before 04.08.08 up to 3.00 p.m. and the same shall be opened on the same day at 3.30 p.m. in the presence of the intending quotationers & their representatives.

Name of work: - Upgradation/ Renovation of existing facility at HNSC.

SH: Painting of Multigym at Pratap Nagar (As per scheduled attached)

**Conditions:**

1. The work/supply should be done at HNSC.
2. The Agency should be professional.
3. The work/supply should be done as per specification.
4. Nothing extra shall be paid.
5. The payment will be made to the agency after the entire satisfaction of Secretary (HNSC) / JE (Civil), HNSC.
6. The undersigned reserves the right to reject /accept the lowest quotations without assigning any reason.
7. The Agency will be responsible for any loss of materials / damage due to negligence.
8. Conditional quotations will not be entertained.
9. The time allowed for execution of the work is 45 days from the date of issue of the work order.
10. The rates shall be inclusive of all taxes including statutory liabilities.
11. Agency should be registered with Trade & Taxes GNCT of Delhi and supposed to furnish a copy of TIN and clearance certificate on Quarterly basis otherwise Quotation may not be considered.
12. Validity of quotation shall be 60 days from the date of opening.

Secretary (HNSC)

CC:

1. Director (Sports).
2. Director (System) with the request to bring the NIQ on DDA’s Web-site through Email- ddatender@dda.org.in.
3. Sr. A.O (Sports).
4. Secretary all sports complexes.
5. A.A.O (HNSC)
6. DDA Contractor Association, Vikas Kutir Room no. 12, Bkno.1, New Delhi.
7. The Secy., DDA Builders Association F-18, Vikas Mina, ITO, New Delhi.
8. DDA Contractor Association E-18 Vikas Kutir, ITO, New Delhi.
9. Notice Board.
10. Guard file

Secretary (HNSC)

**DELHI DEVELOPMENT AUTHORITY**

# HARI NAGAR SPORTS COMPLEX

**Name of work :- M/o Hari Nagar Sports Complex**

**SH : Painting of Multi-Gym at Partap Nagar**

|  |  |  |  |
| --- | --- | --- | --- |
| **Sr. No.** | **Description of Items** | **Qty** | **Unit** |
| 1. | Distempering with oil bound washable distemper of approved brand and manufacture to give an even shade.   1. New work (two or more coats) over and i/c primer cost with cement primer. | 511 | Sqm. |
| 2. | Finishing walls with water proofing cement paint of required shade   1. Old work (one or more coats applied @ 2.20Kg/10 sqm) over priming coat of primer applied @ 0.80 litrs / 10 sqm complete including cost of priming coat. | 777 | Sqm. |
| 3. | Painting with Synthetic enamel paint of approved brand and manufacture of required colour to give an even shade.   1. One or more coats on old work. | 56 | Sqm. |
| 4. | Repairs to plaster of thickness 12mm to 20 mm in patches of area 2.5 sq. meters and under including cutting the patch in proper shape, raking out joints and preparing and plastering the surface of the walls complete including disposal of rubbish to the dumping ground within 50 mtr. Lead.   1. With cement mortar 1:4 (1 cement 4 fine sand) | 5.0 | Sqm. |
| 5. | Renewing glass panes, with putty and nails wherever necessary   1. Float glass panes of thickness 4 mm | 6.30 | Sqm |
| 6. | P/F in position collapsible steel shutters with vertical channels 20 X 10 X 2 mm and braced with flat iron diagonals 20 X 5 mm size with top & bottom rail of T-iron 40 X 40 X 6 mm with 40 mm dia, steel pulleys complete with bolts, nuts, locking arrangement, stoppers, handles i/c applying a priming coat of approved steel primer. | 5.00 | Sqm |
| 7 | Remixing white or color wash by scarping and preparing the surface smooth i/c necessary repairs to scratches etc complete. | 511.00 | Sqm |

**Secretary (HNSC) JE (C)**